/*
   Neo Leaf Panel Project - Clear Diffuser
   
   Measurements in millimeters
   
   Concept, Design and Implementation: Craig A. Lindley
   Last Update: 12/06/2021
*/


$fa = 1;
$fs = 0.4;

// Diffuser thickness
thickness = 1.5;

// Diffuser is made from a polygon and vertically extruded

p = [[-61.5,0],[61.5,0],[69.25,14],[8,121],[-8,121],[-69.25,14]];


module diffuser() {
    linear_extrude(height=thickness)
    translate([0, -60.5,0])
      polygon(p);
}

diffuser();
